Live manual Debian Live

# Debian Live Manual

# O básico

155

# 4. O básico

156

This chapter contains a brief overview of the build process and instructions for using the three most commonly used image types. The most versatile image type, `iso-hybrid`, may be used on a virtual machine, optical medium or USB portable storage device. In certain special cases, as explained later, the `hdd` type may be more suitable. The chapter includes detailed instructions for building and using a `netboot` type image, which is a bit more involved due to the setup required on the server. This is an slightly advanced topic for anyone who is not already familiar with netbooting, but it is included here because once the setup is done, it is a very convenient way to test and deploy images for booting on the local network without the hassle of dealing with image media.

157

The section finishes with a quick introduction to webbooting which is, perhaps, the easiest way of using different images for different purposes, switching from one to the other as needed using the internet as a means.

158

Throughout the chapter, we will often refer to the default filenames produced by live-build. If you are downloading a prebuilt image instead, the actual filenames may vary.

159

4.1 O que é um sistema live?

160

Um sistema live normalmente significa um sistema operacional inicializado em um computador a partir de uma mídia removível, como um CD-ROM ou dispositivo USB, ou de uma rede, pronto a usar, sem qualquer tipo de instalação na unidade de costume (s), com a auto-configuração feita em tempo de execução (veja Termos).

161

With live systems, it's an operating system, built for one of the supported architectures (currently amd64 and i386). It is made from the following parts:

162

- Imagem do kernel do Linux , normalmente chamada `vmlinuz*`

163

- Initial RAM disk image (initrd) - Imagem do disco RAM inicial: um disco de RAM configurado para a inicialização do Linux, que contém módulos que podem ser necessários para montar a imagem do sistema e alguns scripts para fazê-lo.

164

- System image: The operating system's filesystem image. Usually, a SquashFS compressed filesystem is used to minimize the live system image size. Note that it is read-only. So, during boot the live system will use a RAM disk and 'union' mechanism to enable writing files within the running system. However, all modifications will be lost upon shutdown unless optional persistence is used (see Persistence).

165

- Bootloader: A small piece of code crafted to boot from the chosen medium, possibly presenting a prompt or menu to allow selection of options/configuration. It loads the Linux kernel and its initrd to run with an associated system filesystem. Different solutions can be used, depending on the target medium and format of the filesystem containing the previously mentioned components: isolinux to boot from a CD or DVD in ISO9660 format, syslinux for HDD or USB drive booting from a VFAT partition, extlinux for ext2/3/4 and btrfs partitions, pxelinux for PXE netboot, GRUB for ext2/3/4 partitions, etc.

166

You can use live-build to build the system image from your specifications, set up a Linux kernel, its initrd, and a bootloader to run them, all in one medium-dependant format (ISO9660 image, disk image, etc.).

167

4.2 Primeiros passos: construindo uma imagem ISO híbrida

168

Regardless of the image type, you will need to perform the same basic steps to build an image each time. As a first example, create a build directory, change to that directory and then execute the following sequence of live-build commands to create a basic ISO hybrid image containing a default live system without X.org. It is suitable for burning to CD or DVD media, and also to copy onto a USB stick.

169

The name of the working directory is absolutely up to you, but if you take a look at the examples used throughout live-manual, it is a good idea to use a name that helps you identify the image you are working with in each directory, especially if you are working or experimenting with different image types. In this case you are going to build a default system so let's call it, for example, live-default.

170

$ mkdir live-default && cd live-default

171

Then, run the `lb config` command. This will create a "config/" hierarchy in the current directory for use by other commands:

172

$ lb config

173

No parameters are passed to these commands, so defaults for all of their various options will be used. See The lb config command for more details.

174

Agora que existe a hierarquia "config/", construir a imagem com o comando `lb build`:

175

# lb build

176

This process can take a while, depending on the speed of your computer and your network connection. When it is complete, there should be a `live-image-i386.hybrid.iso` image file, ready to use, in the current directory.

177

Note: If you are building on an amd64 system the name of the resulting image will be `live-image-amd64.hybrid.iso`. Keep in mind this naming convention throughout the manual.

178

4.3 Usando uma imagem live ISO hibrida

179

After either building or downloading an ISO hybrid image, which can be obtained at ‹https://www.debian.org/CD/live/›, the usual next step is to prepare your medium for booting, either CD-R(W) or DVD-R(W) optical media or a USB stick.

180

4.3.1 Queimar uma imagem ISO em um meio físico

181

Burning an ISO image is easy. Just install xorriso and use it from the command-line to burn the image. For instance:

182

# apt-get install xorriso
$ xorriso -as cdrecord -v dev=/dev/sr0 blank=as_needed live-image-i386.hybrid.iso

183

4.3.2 Copiar uma imagem ISO híbrida para um dispositivo USB

184

ISO images prepared with `xorriso`, can be simply copied to a USB stick with the `cp` program or an equivalent. Plug in a USB stick with a size large enough for your image file and determine which device it is, which we hereafter refer to as `${USBSTICK}`. This is the device file of your key, such as `/dev/sdb`, not a partition, such as `/dev/sdb1`! You can find the right device name by looking in `dmesg`'s output after plugging in the stick, or better yet, `ls -l /dev/disk/by-id`.

185

Once you are certain you have the correct device name, use the `cp` command to copy the image to the stick. This will definitely overwrite any previous contents on your stick!

186

$ cp live-image-i386.hybrid.iso ${USBSTICK}
$ sync

187

Note: The sync command is useful to ensure that all the data, which is stored in memory by the kernel while copying the image, is written to the USB stick.

188

4.3.3 Using the space left on a USB stick

189

After copying the `live-image-i386.hybrid.iso` to a USB stick, the first partition on the device will be filled up by the live system. To use the remaining free space, use a partitioning tool such as gparted or parted to create a new partition on the stick.

190

# gparted ${USBSTICK}

191

After the partition is created, where `${PARTITION}` is the name of the partition, such as `/dev/sdb2`, you have to create a filesystem on it. One possible choice would be ext4.

192

# mkfs.ext4 ${PARTITION}

193

Note: If you want to use the extra space with Windows, apparently that OS cannot normally access any partitions but the first. Some solutions to this problem have been discussed on our mailing list, but it seems there are no easy answers.

194

Remember: Every time you install a new live-image-i386.hybrid.iso on the stick, all data on the stick will be lost because the partition table is overwritten by the contents of the image, so back up your extra partition first to restore again after updating the live image.

195

4.3.4 Booting the live medium

196

The first time you boot your live medium, whether CD, DVD, USB key, or PXE boot, some setup in your computer's BIOS may be needed first. Since BIOSes vary greatly in features and key bindings, we cannot get into the topic in depth here. Some BIOSes provide a key to bring up a menu of boot devices at boot time, which is the easiest way if it is available on your system. Otherwise, you need to enter the BIOS configuration menu and change the boot order to place the boot device for the live system before your normal boot device.

197

Once you've booted the medium, you are presented with a boot menu. If you just press enter here, the system will boot using the default entry, `Live` and default options. For more information about boot options, see the "help" entry in the menu and also the live-boot and live-config man pages found within the live system.

198

Assuming you've selected `Live` and booted a default desktop live image, after the boot messages scroll by, you should be automatically logged into the `user` account and see a desktop, ready to use. If you have booted a console-only image, you should be automatically logged in on the console to the `user` account and see a shell prompt, ready to use.

199

4.4 Usando uma máquina virtual para testar

200

It can be a great time-saver for the development of live images to run them in a virtual machine (VM). This is not without its caveats:

201

- Running a VM requires enough RAM for both the guest OS and the host and a CPU with hardware support for virtualization is recommended.

202

- There are some inherent limitations to running on a VM, e.g. poor video performance, limited choice of emulated hardware.

203

- When developing for specific hardware, there is no substitute for running on the hardware itself.

204

- Occasionally there are bugs that relate only to running in a VM. When in doubt, test your image directly on the hardware.

205

Provided you can work within these constraints, survey the available VM software and choose one that is suitable for your needs.

206

4.4.1 Testing an ISO image with QEMU

207

The most versatile VM in Debian is QEMU. If your processor has hardware support for virtualization, use the qemu-kvm package; the qemu-kvm package description briefly lists the requirements.

208

First, install qemu-kvm if your processor supports it. If not, install qemu, in which case the program name is `qemu` instead of `kvm` in the following examples. The qemu-utils package is also valuable for creating virtual disk images with `qemu-img`.

209

# apt-get install qemu-kvm qemu-utils

210

Booting an ISO image is simple:

211

$ kvm -cdrom live-image-i386.hybrid.iso

212

See the man pages for more details.

213

4.4.2 Testing an ISO image with VirtualBox

214

In order to test the ISO with virtualbox:

215

# apt-get install virtualbox virtualbox-qt virtualbox-dkms
$ virtualbox

216

Create a new virtual machine, change the storage settings to use `live-image-i386.hybrid.iso` as the CD/DVD device, and start the machine.

217

Note: For live systems containing X.org that you want to test with virtualbox, you may wish to include the VirtualBox X.org driver package, virtualbox-guest-dkms and virtualbox-guest-x11, in your live-build configuration. Otherwise, the resolution is limited to 800x600.

218

$ echo "virtualbox-guest-dkms virtualbox-guest-x11" >> config/package-lists/my.list.chroot

219

In order to make the dkms package work, also the kernel headers for the kernel flavour used in your image need to be installed. Instead of manually listing the correct linux-headers package in above created package list, the selection of the right package can be done automatically by live-build.

220

$ lb config --linux-packages "linux-image linux-headers"

221

4.5 Building and using an HDD image

222

Building an HDD image is similar to an ISO hybrid one in all respects except you specify `-b hdd` and the resulting filename is `live-image-i386.img` which cannot be burnt to optical media. It is suitable for booting from USB sticks, USB hard drives, and various other portable storage devices. Normally, an ISO hybrid image can be used for this purpose instead, but if you have a BIOS which does not handle hybrid images properly, you need an HDD image.

223

Note: if you created an ISO hybrid image with the previous example, you will need to clean up your working directory with the `lb clean` command (see The lb clean command):

224

# lb clean --binary

225

Run the `lb config` command as before, except this time specifying the HDD image type:

226

$ lb config -b hdd

227

Now build the image with the `lb build` command:

228

# lb build

229

When the build finishes, a `live-image-i386.img` file should be present in the current directory.

230

The generated binary image contains a VFAT partition and the syslinux bootloader, ready to be directly written on a USB device. Once again, using an HDD image is just like using an ISO hybrid one on USB. Follow the instructions in Using an ISO hybrid live image, except use the filename `live-image-i386.img` instead of `live-image-i386.hybrid.iso`.

231

Likewise, to test an HDD image with Qemu, install qemu as described above in Testing an ISO image with QEMU. Then run `kvm` or `qemu`, depending on which version your host system needs, specifying `live-image-i386.img` as the first hard drive.

232

$ kvm -hda live-image-i386.img

233

4.6 Building a netboot image

234

The following sequence of commands will create a basic netboot image containing a default live system without X.org. It is suitable for booting over the network.

235

Note: if you performed any previous examples, you will need to clean up your working directory with the `lb clean` command:

236

# lb clean

237

In this specific case, a `lb clean --binary` would not be enough to clean up the necessary stages. The cause for this is that in netboot setups, a different initramfs configuration needs to be used which live-build performs automatically when building netboot images. Since the initramfs creation belongs to the chroot stage, switching to netboot in an existing build directory means to rebuild the chroot stage too. Therefore, `lb clean` (which will remove the chroot stage, too) needs to be used.

238

Run the `lb config` command as follows to configure your image for netbooting:

239

$ lb config -b netboot --net-root-path "/srv/debian-live" --net-root-server "192.168.0.2"

240

In contrast with the ISO and HDD images, netbooting does not, itself, serve the filesystem image to the client, so the files must be served via NFS. Different network filesystems can be chosen through lb config. The `--net-root-path` and `--net-root-server` options specify the location and server, respectively, of the NFS server where the filesystem image will be located at boot time. Make sure these are set to suitable values for your network and server.

241

Now build the image with the `lb build` command:

242

# lb build

243

In a network boot, the client runs a small piece of software which usually resides on the EPROM of the Ethernet card. This program sends a DHCP request to get an IP address and information about what to do next. Typically, the next step is getting a higher level bootloader via the TFTP protocol. That could be pxelinux, GRUB, or even boot directly to an operating system like Linux.

244

For example, if you unpack the generated `live-image-i386.netboot.tar` archive in the `/srv/debian-live` directory, you'll find the filesystem image in `live/filesystem.squashfs` and the kernel, initrd and pxelinux bootloader in `tftpboot/`.

245

We must now configure three services on the server to enable netbooting: the DHCP server, the TFTP server and the NFS server.

246

4.6.1 Servidor DHCP

247

We must configure our network's DHCP server to be sure to give an IP address to the netbooting client system, and to advertise the location of the PXE bootloader.

248

Here is an example for inspiration, written for the ISC DHCP server `isc-dhcp-server` in the `/etc/dhcp/dhcpd.conf` configuration file:

249

# /etc/dhcp/dhcpd.conf - configuration file for isc-dhcp-server
ddns-update-style none;
option domain-name "example.org";
option domain-name-servers ns1.example.org, ns2.example.org;
default-lease-time 600;
max-lease-time 7200;
log-facility local7;
subnet 192.168.0.0 netmask 255.255.255.0 {
range 192.168.0.1 192.168.0.254;
filename "pxelinux.0";
next-server 192.168.0.2;
option subnet-mask 255.255.255.0;
option broadcast-address 192.168.0.255;
option routers 192.168.0.1;
}

250

4.6.2 Servidor TFTP

251

This serves the kernel and initial ramdisk to the system at run time.

252

You should install the tftpd-hpa package. It can serve all files contained inside a root directory, usually `/srv/tftp`. To let it serve files inside `/srv/debian-live/tftpboot`, run as root the following command:

253

# dpkg-reconfigure -plow tftpd-hpa

254

and fill in the new tftp server directory when being asked about it.

255

4.6.3 Servidor NFS

256

Once the guest computer has downloaded and booted a Linux kernel and loaded its initrd, it will try to mount the Live filesystem image through a NFS server.

257

You need to install the nfs-kernel-server package.

258

Then, make the filesystem image available through NFS by adding a line like the following to `/etc/exports`:

259

/srv/debian-live *(ro,async,no_root_squash,no_subtree_check)

260

and tell the NFS server about this new export with the following command:

261

# exportfs -rv

262

Setting up these three services can be a little tricky. You might need some patience to get all of them working together. For more information, see the syslinux wiki at ‹https://wiki.syslinux.org/wiki/index.php?title=PXELINUX› or the Debian Installer Manual's TFTP Net Booting section at ‹https://www.debian.org/releases/stable/i386/ch04s05.en.html›. They might help, as their processes are very similar.

263

4.6.4 Netboot testing HowTo

264

Netboot image creation is made easy with live-build, but testing the images on physical machines can be really time consuming.

265

To make our life easier, we can use virtualization.

266

4.6.5 Qemu

267

- Install qemu, bridge-utils, sudo.

268

Edit `/etc/qemu-ifup`:

269

#!/bin/sh
sudo -p "Senha para $0:" /sbin/ifconfig $1 172.20.0.1
echo "Executando /etc/qemu-ifup"
echo "Levando o $1 para o modo bridged..."
sudo /sbin/ifconfig $1 0.0.0.0 promisc up
echo "Adicionando $1 to br0..."
sudo /usr/sbin/brctl addif br0 $1
sleep 2

270

Get, or build a `grub-floppy-netboot`.

271

Launch `qemu` with "`-net nic,vlan=0 -net tap,vlan=0,ifname=tun0`"

272

4.7 Webbooting

273

Webbooting is a convenient way of retrieving and booting live systems using the internet as a means. The requirements for webbooting are very few. On the one hand, you need a medium with a bootloader, an initial ramdisk and a kernel. On the other hand, a web server to store the squashfs files which contain the filesystem.

274

4.7.1 Getting the webboot files

275

As usual, you can build the images yourself or use the prebuilt files, which are available on the project's download page at ‹https://www.debian.org/CD/live/›. Using prebuilt images would be handy for doing initial testing until one can fine tune their own needs. If you have built a live image you will find the files needed for webbooting in the build directory under `binary/live/`. The files are called `vmlinuz`, `initrd.img` and `filesystem.squashfs`.

276

It is also possible to extract those files from an already existing iso image. In order to achieve that, loopback mount the image as follows:

277

# mount -o loop image.iso /mnt

278

The files are to be found under the `live/` directory. In this specific case, it would be `/mnt/live/`. This method has the disadvantage that you need to be root to be able to mount the image. However, it has the advantage that it is easily scriptable and thus, easily automatized.

279

But undoubtedly, the easiest way of extracting the files from an iso image and uploading it to the web server at the same time, is using the midnight commander or mc. If you have the genisoimage package installed, the two-pane file manager allows you to browse the contents of an iso file in one pane and upload the files via ftp in the other pane. Even though this method requires manual work, it does not require root privileges.

280

4.7.2 Booting webboot images

281

While some users will prefer virtualization to test webbooting, we refer to real hardware here to match the following possible use case which should only be considered as an example.

282

In order to boot a webboot image it is enough to have the components mentioned above, i.e. `vmlinuz` and `initrd.img` in a usb stick inside a directory named `live/` and install syslinux as bootloader. Then boot from the usb stick and type `fetch=URL/PATH/TO/FILE` at the boot options. live-boot will retrieve the squashfs file and store it into ram. This way, it is possible to use the downloaded compressed filesystem as a regular live system. For example:

283

append boot=live components fetch=http://192.168.2.50/images/webboot/filesystem.squashfs

284

Use case: You have a web server in which you have stored two squashfs files, one which contains a full desktop, like for example gnome, and a standard one. If you need a graphical environment for one machine, you can plug your usb stick in and webboot the gnome image. If you need one of the tools included in the second type of image, perhaps for another machine, you can webboot the standard one.